/* 20-bit address */
PARTIAL_INT_MODE (SI, 20, PSI);

INT_N (PSI, 20);
